Lever sets for standard doors acc. to DIN EN 1906, category of use 3
Lever version ER18 Rhodos XL
by KARCHER DESIGN

Solid 3-piece fixing rose
and escutcheons squared, 52 x 10 mm,
with 7mm lugs and nylon floating bearing,
sprung loaded inner plate with attached lever
Heavy duty bolt through M4 fixings
8mm offset drilled spindle,		
diameter of handle: 22 mm, middle value of handle diameter
standard door thickness: 39-47 mm

Options:

OS (without escutcheon)
BB (key hole),
PZ (Euro profile)
BAD (turn & release)

Finish: satin stainless steel 
Karcher article no.:

ER18 OS 71 (without escutcheon)
ER18 BB0 71 (key hole)
ER18 PZ0 71 (Euro profile)
ER18 BAD 71 (turn &release

Dimensional detail:

60

131

22