Lever sets for standard doors acc. to DIN EN 1906, category of use 3
Lever version ER25 Malta
Lever sets for projects acc. to DIN EN 1906, category of use 4
Lever version ER/EN 25 Malta
by KARCHER DESIGN

Solid 3-piece fixing rose
and escutcheons squared, 52 x 10 mm,
with 7mm lugs and nylon floating bearing,
sprung loaded inner plate with attached lever
Heavy duty bolt through M4 fixings
8mm offset drilled spindle,
diameter of handle: 19 mm 
standard door thickness: 39 - 47 mm

Options:
OS – without escutcheon
BB – supplied with lever key escutcheons
PZ – supplied with euro profile escutcheons
BAD – supplied with bathroom turn/release set
EN – supplied according to DIN EN 1906, category of use 4, OS, BB, PZ
FS – supplied as fire-resisting set

Finish: satin stainless steel (finish code 71)
Karcher article no.:
ER25 OS 71 – without escutcheon
ER25 BB0 71 – supplied with lever key escutcheons
ER25 PZ0 71 – supplied with euro profile escutcheons
ER25 BAD 71 – supplied with bathroom turn/release set
ER/EN25 71 – supplied acc. to DIN EN 1906, category of use 4
ER/FS25 PZ0 71 – supplied of fire resisting set

Dimensional detail:

130 mm

60

19