Security lever set 
Model ESG685K
burglary insurance category ES3 after DIN 18257
Category of use 4 and security class 4 after DIN EN 1906
by KARCHER DESIGN

Options:
ESG685K with cylinder protection as knob/lever set
ESG685KF with cylinder protection as fire-resisting set
Outside plate 255 x 53 x 15 mm
with cranked knob
Solid sandwich architecture with 12 mm lugs and
invisible triple screwing
Inner plate 255 x 53 x 5 mm
Lever by choice
nylon floating bearing,
Sprung loaded inner plate with attached lever
optional with return to door handle 
(project building)
8 mm respectively 8/10 mm offset drilled spindle, 
standard door thickness: 39 - 43 mm
Euro profile PZ72 mm or PZ92 mm

Finish: satin stainless steel (finish code 71)
Karcher article no.:
ESG685K PZ 71 
ESG685KF PZ 71 
Optional with lever ER20 - ER30, ER32, ER34, ER35, ER37 and ER43
Higher price category for lever models ER31, ER33, ER36, ER44 – ER84

Due to fixing reasons not all lever sets are connected fix with the plate.

255

53

139

76

21,5

Dimensional detail: