Sliding door kit EPD 
by KARCHER DESIGN

Options: 
EPD3 :  
Outside rose with slot, inside rose with thumb turn, 8mm spindle, finger pull, including lock (backset 49,5mm), with strike plate, standard door thickness (45mm)

EPD3 0S : 
Blind Roses inside and outside, finger pull

Finish: satin stainless steel, polished stainless steel, oil rubbed bronze, cosmos black.
Dimensions: Ø  60 mm x 12 mm

Karcher article no.:
EPD3 71
EPD3 72
EPD3 81
EPD3 83

EPD3 0S 71
EPD3 0S 72 
EPD3 OS 81
EPD3 OS 83

Dimensional details:

Attention: The measures in this sheet are not supposed to be used for milling.